In addition to the raspberry pi being able to inject programs into ram, and a keyboard which generates user input, I plan on adding a manual override to the control unit. Instead of a manual switch as used in the past, an octal bus transfer can be utilized for faster switching.